Folder Structure:
|Acro Series
	|Long
		|Glass Lens
		|PC Lens
	|Short
		|Glass Lens
		|PC Lens

File name structure

Acro Mini YYYYY Size BB CCXX FF.LDT
--------- ----- ---- -- ---- --
|	  |	|    |  |    |Finish colour
|	  |	|    |  |CCT + CRI
|	  |	|    |Beam angle
|	  |	|Shape/Size
|	  |Accessory or lens material
|Family Name


Accessory or Lens material
Standard PC lens
Glass = Glass Lens
HC = PC lens + Honeycomb

Shape/Size
Long or Short

Beam Angle
10 = 10° (only available in PC)
20 = 20° (only available in PC)
40 = 40° (available in glass and PC)
60 = 60° (only available in PC)

CC
27 = 2700K
30 = 3000K
35 = 3500K
40 = 4000K

XX
90 = CRI90
97 = CRI97

Finish colour
BA  = Black Anodized
BB  = Brushed Bronze
BG  = Brushed Grey
BN  = Brushed Nickle
BS  = Brushed Steel
CFD = Canon Fusil Dark
CFL = Canon Fusil Light
DB  = Dark Bronze
LB  = Light Bronze
WS  = White Structure

