Folder Structure:
|adjustable spot series
	|glass optics 40°
	|pc optics 20°-60°

All files are applicable for Trim & Trimless

File name structure

Acro Mini YYYYY BB CCXX FF-xxxmA.IES
--------- ----- -- ---- -- ---
|	  |	|  |	|  |Current setting in mA
|	  |	|  |    |Finish colour
|	  |	|  |CCT + CRI
|	  |	|Beam angle
|	  |Accessory or lens material
|Family Name


Accessory or Lens material
Standard PC lens
Glass = Glass Lens


Beam Angle
20 = 20° (only available in PC)
40 = 40° (available in glass and PC)
60 = 60° (only available in PC)

CC
24 = 2400K
27 = 2700K
30 = 3000K
35 = 3500K
40 = 4000K
1830 = Dim 2 Warm 3000K to 1800K

XX
90 = CRI90
97 = CRI97

Finish colour
BA  = Black Anodized
BB  = Brushed Bronze
BG  = Brushed Grey
BN  = Brushed Nickle
BS  = Brushed Steel
CFD = Canon Fusil Dark
CFL = Canon Fusil Light
DB  = Dark Bronze
LB  = Light Bronze
WS  = White Structure

